**Energy Efficiency Compliant Products - EEPLIANT3 [GA: 832558]**

**WP10 Concerted market surveillance action for product group "Ventilation Units"**

**ANNEX C** **Financial proposal**

**Call for Tenders for Laboratory Test Services**

|  |
| --- |
| **The offer concerns** |
| **Product category** |
| Bidirectional central RVU with heat recovery. | ☐ |
| Bidirectional decentral RVU with heat recovery. | ☐ |
| Alternating (push-pull) bidirectional decentral RVU with heat recovery. | ☐ |
| Unidirectional central RVU. | ☐ |
| Unidirectional decentral RVU | ☐ |
| **Capacity range**  |
| Maximum flow rate ≤ 450 m3/h  | ☐ |
|  Maximum flow rate 450 m3/h to 1000 m3/h  | ☐ |

Unit cost should be quoted in Euros excluding VAT.

Unit cost must include the ‘testing services'. ‘Testing services’ means the following (see also Annex B: Requirements):

* Planning of testing programme;
* Receipt of products and storage;
* Discussions and suggestions on screening tests and stop/go criteria during test.
* Storage after test until disposal or end of contract (see assumptions above regarding this);
* Photos of products;
* Potentially preinspection of the product (only relevant for Annex C, unit cost group 2);
* Testing of each product as specified. Any significant differences in the price of testing due to different possible standards should be explained in the proposal and if necessary costed separately;
* Standard report for each product as agreed but based on that in the harmonised standard (or standards named or methods described in the transitional methods);
* Separate report on circumvention checks, compliance recommendation etc. as described in requirements section above;
* Meeting(s) including physical at the test lab and virtual meetings to discuss the test programme, testing progress, and the test results as per requirements in Annex C;
* Project management etc.
* Final report.

**Unit costs per group of test parameters**

| **Tested Parameter** | **ED or EL Information or Minimum require­ment?****(I/M)** | **Reference** | **Unit cost****(EUR Excl VAT)** |
| --- | --- | --- | --- |
| **Single-product testing 1-4 samples** | **Single-product testing5 or more samples** | **Triple-product testingof one sample** |
| **Group 1** |
| **SPI** – Specific power input [W/(m3/s)] | I | Regulation 1253/2014 Annex I (13)  |  |  |  |
| Thermal Effi­ciency (*η*t) of heat recovery | I | Regulation 1253/2014 Annex 1 (6) |
| Electric power input of fan incl. motor con­trol equipment, *P*E,ref, [W] | I | Regulation 1253/2014 Annex 1 (6) |
| Sound Power Level(*L*WA) | M (non-ducted)I (all RVUs) | Regulation 1253/2014 Annex 1 (2) |  |  |  |
| Maximum flow rate [m3/h] Declared value according to flow rate/pressure diagrams. Verify that it can be reached  | I | Regulation 1253/ 2014 Annex I (14) and Annex IV (k) |  |  |  |
| **Group 2 - will only be requested together with Group 1 tests and not as stand-alone tests.** |
| **SEC** — Specific Energy Consump­tion for ventilation per m2 heated floor area of a dwelling or building [kWh/(m2.a)]Calculate for each applicable climate zone. | M | Regulation 1253/ 2014 Annex VIIIand Regulation 1254/ 2014 Annex VIII |  |  |  |
| Type of drive installed: Multi speed drive or VSD?Verify correctness | I | Regulation 1253/ 2014 Annex I (3)and Regulation 1254/ 2014 Annex I (3) |
| Thermal bypass (BVU)Verify correctness | M | Regulation 1253/ 2014 Annex I (35) |
| Visual filter change warning signalVerify correctness | M | Regulation 1253/ 2014 Annex II (2) |
| Declared typology (RVU/NRVU, UVU/BVU)Verify correctness  | I | Regulation 1253/ 2014 Article 2 and Annex I (22) and (23) |
| Type of heat recovery system (HRS)Verify correctness | I | Regulation 1253/ 2014 Annex I (5) and (13) |
| Control factor and typologyVerify correctness  | I | Regulation 1253/ 2014 Annex I (16) to (21) |
| Instructions for disassembly etc.Verify correctness | I | Regulation 1253/2014 Annex IV (s) |  |  |  |
| **Group 3 – Verification tests which will only be requested together with Group 1 tests and not as stand-alone tests.** |
| External total pressure difference | n.a. | Commission Communication in OJ 2016/C 416/06[[1]](#footnote-2) article 2.2  |  |  |  |
| Reference flow rate [m3/s] and flow rate/pressureDiagramMeasure and verify correctness | I | Regulation 1253/ 2014 Annex I (14) and (15)Commission Communica­tion3 article 2.2 and 3 |  |  |  |
| Max. internal leakage rate,  | I(BVU, ducted) | Regulation 1253/ 2014 Annex I (7)  |  |  |  |
| Max. external leakage rates  | I(BVU and ducted UVU, regenerative heat exch., ducted) | Regulation 1253/ 2014 Annex I (9)  |
| Mixing rate  | I (non-ducted BVU) | Regulation 1253/ 2014 Annex I (10) |  |  |  |
| The airflow sensitivity to pressure variations at +20 Pa and -20 Pa; | I(non-ducted) | Regulation 1253/ 2014 Annex I (32) |  |  |  |
| The indoor/outdoor air tightness in m3/h | I(non-ducted) | Regulation 1253/ 2014 Annex I (33) |  |  |  |

**Other costs**

|  |  |
| --- | --- |
| Cost for disposal of product per unit  | Euros:  |
| Discount if more than 10 products are tested Example.  6 nonducted UVUs below 450 m3/h + 8 ducted BVUs below 450 m3/h + 5 ducted BVUs above 450 m3/h= 19 unitsThe 15 cheapets units will be prices according to prices informend in the financial offer above, and the 4 most expensive with the informed discount rate  |  Dicsount rate in % for more than 15 units:  |

**Hourly rate in case of purchase of additional services**

|  |  |  |
| --- | --- | --- |
| **Name of team member** | **Job title/function of team member** | **Hourly rate (Euros)** |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Full name Date Signature**

**DISCLAIMER**

This tender is part of the EEPLIANT3 concerted action that has received funding from the European Union’s Horizon 2020 research and innovation programme under grant agreement No 832558.

The content of this tender represents the views of the author and it is his sole responsibility; it can in no way be taken to reflect the views of the European Climate, Infrastructure and Environment Executive Agency (CINEA), the European Commission or any other body of the European Union, who are not responsible for any use that may be made of the information it contains.

1. *Commission communication in the framework of the implementation of Commission Regulation (EU) No 1253/2014 implementing Directive 2009/125/EC of the European Parliament and of the Council with regard to ecodesign requirements for ventilation units and of the implementation of Commission Delegated Regulation (EU) No 1254/2014 supplementing Directive 2010/30/EU of the European Parliament and of the Council with regard to energy labelling of residential ventilation unit*, https://eur-lex.europa.eu/legal-content/EN/TXT/PDF/?uri=CELEX:52016XC1111(09)&from=EN [↑](#footnote-ref-2)